<?xml version="1.0" encoding="UTF-8"?>
<!--
  Licensed to the Apache Software Foundation (ASF) under one or more
  contributor license agreements.  See the NOTICE file distributed with
  this work for additional information regarding copyright ownership.
  The ASF licenses this file to You under the Apache License, Version 2.0
  (the "License"); you may not use this file except in compliance with
  the License.  You may obtain a copy of the License at

      http://www.apache.org/licenses/LICENSE-2.0

  Unless required by applicable law or agreed to in writing, software
  distributed under the License is distributed on an "AS IS" BASIS,
  WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  See the License for the specific language governing permissions and
  limitations under the License.
-->
<!DOCTYPE document [
  <!ENTITY project SYSTEM "project.xml">
]>
<document url="cluster-membership.html">

  &project;

  <properties>
    <author email="fhanik@apache.org">Filip Hanik</author>
    <title>The Cluster Membership object</title>
  </properties>

<body>

<section name="Table of Contents">
<toc/>
</section>

<section name="Introduction">
  <p>
    The membership component in the Apache Tribes <a href="cluster-channel.html">Channel</a> is responsible
    for dynamic discovery of other members(nodes) in the cluster.
    There are currently two different membership service, the <code>org.apache.catalina.tribes.membership.McastService</code>
    and the <code>org.apache.catalina.tribes.membership.StaticMembershipService</code>.
    The <code>McastService</code> builds a multicast based membership service
    that sends UDP packets to multicast IP addresses.
    The <code>StaticMembershipService</code> builds  a unicast based membership
    service that sends TCP packets to predefined member address.
  </p>
</section>

<section name="Default Implementation">
  <p>
    The default implementation of the cluster group notification is built on top of multicast heartbeats
    sent using UDP packets to a multicast IP address.
    Cluster members are grouped together by using the same multicast address/port combination.
    Each member sends out a heartbeat with a given interval (<code>frequency</code>), and this
    heartbeat is used for dynamic discovery.
    In a similar fashion, if a heartbeat has not been received in a timeframe specified by <code>dropTime</code>
    ms. a member is considered suspect and the channel and any membership listener will be notified.
  </p>
</section>



<section name="Attributes">
  <subsection name="Common Attributes">
    <attributes>
      <attribute name="className" required="true">
        <p>
        The implementation of the membership component.
        Two implementations available, <code>org.apache.catalina.tribes.membership.McastService</code>
        and <code>org.apache.catalina.tribes.membership.StaticMembershipService</code>.
        </p>
      </attribute>
    </attributes>
  </subsection>
  <subsection name="Multicast Attributes">

  <attributes>

    <attribute name="className" required="true">
      <p>
      The value is <code>org.apache.catalina.tribes.membership.McastService</code>.
      This implementation uses multicast heartbeats for member discovery.
      </p>
    </attribute>
    <attribute name="address" required="false">
      <p>
      The multicast address that the membership will broadcast its presence and listen
      for other heartbeats on. The default value is <code>228.0.0.4</code>
      Make sure your network is enabled for multicast traffic.<br/>
      The multicast address, in conjunction with the <code>port</code> is what
      creates a cluster group. To divide up your farm into several different group, or to
      split up QA from production, change the <code>port</code> or the <code>address</code>
      <br/>Previously known as mcastAddr.
      </p>
    </attribute>
    <attribute name="port" required="false">
      <p>
      The multicast port, the default value is <code>45564</code><br/>
      The multicast port, in conjunction with the <code>address</code> is what
      creates a cluster group. To divide up your farm into several different group, or to
      split up QA from production, change the <code>port</code> or the <code>address</code>
      </p>
    </attribute>
    <attribute name="frequency" required="false">
      <p>
      The frequency in milliseconds in which heartbeats are sent out. The default value is <code>500</code> ms.<br/>
      In most cases the default value is sufficient. Changing this value, simply changes the interval in between heartbeats.
      </p>
    </attribute>
    <attribute name="dropTime" required="false">
      <p>
      The membership component will time out members and notify the Channel if a member fails to send a heartbeat within
      a give time. The default value is <code>3000</code> ms. This means, that if a heartbeat is not received from a
      member in that timeframe, the membership component will notify the cluster of this.<br/>
      On a high latency network you may wish to increase this value, to protect against false positives.<br/>
      Apache Tribes also provides a <a href="cluster-interceptor.html#org.apache.catalina.tribes.group.interceptors.TcpFailureDetector_Attributes"><code>TcpFailureDetector</code></a> that will
      verify a timeout using a TCP connection when a heartbeat timeout has occurred. This protects against false positives.
      </p>
    </attribute>
    <attribute name="bind" required="false">
      <p>
      Use this attribute if you wish to bind your multicast traffic to a specific network interface.
      By default, or when this attribute is unset, it tries to bind to <code>0.0.0.0</code> and sometimes on multihomed hosts
      this becomes a problem.
      </p>
    </attribute>
    <attribute name="ttl" required="false">
      <p>
      The time-to-live setting for the multicast heartbeats.
      This setting should be a value between 0 and 255. The default value is VM implementation specific.
      </p>
    </attribute>
    <attribute name="domain" required="false">
      <p>
      Apache Tribes has the ability to logically group members into domains, by using this domain attribute.
      The <code>org.apache.catalina.tribes.Member.getDomain()</code> method returns the value specified here.
      </p>
    </attribute>
    <attribute name="soTimeout" required="false">
      <p>
      The sending and receiving of heartbeats is done on a single thread, hence to avoid blocking this thread forever,
      you can control the <code>SO_TIMEOUT</code> value on this socket.<br/>
      If a value smaller or equal to 0 is presented, the code will default this value to frequency
      </p>
    </attribute>
    <attribute name="recoveryEnabled" required="false">
      <p>
      In case of a network failure, Java multicast socket don't transparently fail over, instead the socket will continuously
      throw IOException upon each receive request. When recoveryEnabled is set to true, this will close the multicast socket
      and open a new socket with the same properties as defined above.<br/>
      The default is <code>true</code>. <br/>
      </p>
    </attribute>
    <attribute name="recoveryCounter" required="false">
      <p>
      When <code>recoveryEnabled==true</code> this value indicates how many
      times an error has to occur before recovery is attempted. The default is
      <code>10</code>. <br/>
      </p>
    </attribute>
    <attribute name="recoverySleepTime" required="false">
      <p>
      When <code>recoveryEnabled==true</code> this value indicates how long time (in milliseconds)
      the system will sleep in between recovery attempts, until it recovers successfully.
      The default is <code>5000</code> (5 seconds). <br/>
      </p>
    </attribute>

    <attribute name="localLoopbackDisabled" required="false">
      <p>
      Membership uses multicast, it will call <code>java.net.MulticastSocket.setLoopbackMode(localLoopbackDisabled)</code>.
      When <code>localLoopbackDisabled==true</code> multicast messages will not reach other nodes on the same local machine.
      The default is <code>false</code>. <br/>
      </p>
    </attribute>

  </attributes>

  </subsection>

  <subsection name="Static Membership Attributes">
    <attributes>
      <attribute name="className" required="true">
        <p>
        The value is <code>org.apache.catalina.tribes.membership.StaticMembershipService</code>.
        </p>
      </attribute>
      <attribute name="connectTimeout" required="false">
        <p>
        Timeout for attempting a TCP connection to address of predefined static member.
        Default is <code>500</code> ms.
        </p>
      </attribute>
      <attribute name="expirationTime" required="false">
        <p>
        If members have failed to update their alive time within the given time,
        this membership will notify the memberDisappeared event to cluster.
        Default is <code>5000</code> ms.
        </p>
      </attribute>
      <attribute name="rpcTimeout" required="false">
        <p>
        Timeout for messages that used for member notification to/from othee nodes.
        Default is <code>3000</code> ms.
        </p>
      </attribute>
      <attribute name="useThread" required="false">
        <p>
        If set to true, this membership service will start a local thread for
        sending a ping message. if set to <code>false</code>, channel heartbeat
        will send a ping message. Default is <code>false</code>.
        </p>
      </attribute>
      <attribute name="pingInterval" required="false">
        <p>
        If <code>useThread</code> == <code>true</code>, defines the interval of
        sending a ping message. Default is <code>1000</code> ms.
        </p>
      </attribute>
    </attributes>
  </subsection>

</section>

<section name="Nested Components">
  <p>
  Static Membership Service allows nesting of a <strong>&lt;LocalMember&gt;</strong>
  and <strong>&lt;Member&gt;</strong>element.
  </p>
  <subsection name="StaticMember Attributes">
    <p><b>LocalMember:</b> <br/>
    Static member that is the local member of the static cluster group.
    </p>
    <attributes>
      <attribute name="className" required="true">
        Only one implementation available:<code>org.apache.catalina.tribes.membership.StaticMember</code>
      </attribute>
      <attribute name="port" required="false">
        There is no need to set.
        The value of this attribute inherits from the cluster receiver setting.
      </attribute>
      <attribute name="securePort" required="false">
        There is no need to set.
        The value of this attribute inherits from the cluster receiver setting.
      </attribute>
      <attribute name="host" required="false">
        There is no need to set.
        The value of this attribute inherits from the cluster receiver setting.
      </attribute>
      <attribute name="domain" required="false">
        The logical cluster domain for that this static member listens for cluster messages.
        Two different type of values are possible:<br/>
        1. Regular string values like &quot;staging-domain&quot; or &quot;tomcat-cluster&quot; will be converted into bytes
        using ISO-8859-1 encoding.
        2. byte array in string form, for example {216,123,12,3}<br/>
      </attribute>
      <attribute name="uniqueId" required="true">
        A universally uniqueId for this static member.
        The values must be 16 bytes in the following form:<br/>
        1. byte array in string form, for example {0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15}<br/>
      </attribute>
    </attributes>

    <p><b>Member:</b> <br/>
    Static member that add to the static cluster group.
    </p>
    <attributes>
      <attribute name="className" required="true">
        Only one implementation available:<code>org.apache.catalina.tribes.membership.StaticMember</code>
      </attribute>
      <attribute name="port" required="true">
        The port that this static member listens to for cluster messages
      </attribute>
      <attribute name="securePort" required="false">
        The secure port this static member listens to for encrypted cluster messages
        default value is <code>-1</code>, this value means the member is not listening on a secure port
      </attribute>
      <attribute name="host" required="true">
        The host (or network interface) that this static member listens for cluster messages.
        Three different type of values are possible:<br/>
        1. IP address in the form of &quot;216.123.1.23&quot;<br/>
        2. Hostnames like &quot;tomcat01.mydomain.com&quot; or &quot;tomcat01&quot; as long as they resolve correctly<br/>
        3. byte array in string form, for example {216,123,12,3}<br/>
      </attribute>
      <attribute name="domain" required="false">
        The logical cluster domain for that this static member listens for cluster messages.
        Two different type of values are possible:<br/>
        1. Regular string values like &quot;staging-domain&quot; or &quot;tomcat-cluster&quot; will be converted into bytes
        using ISO-8859-1 encoding.<br/>
        2. byte array in string form, for example {216,123,12,3}<br/>
      </attribute>
      <attribute name="uniqueId" required="true">
        A universally uniqueId for this static member.
        The values must be 16 bytes in the following form:<br/>
        1. byte array in string form, for example {0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15}<br/>
      </attribute>
    </attributes>
  </subsection>
</section>

</body>

</document>
